
**IP20**

**TECHNICAL IMAGE**



**DESIGN** **BY**

Emilux Lighting Limited

**DESCRIPTION**

* Multi power for commercial and architectural lighting
* Average lighting with die-casting Aluminium material
* Average performance within different dimension
* External dimming system: Triac/ 0-10V/ Dali/Bluetooth/ Tuya/ Zigbee

|  |  |  |
| --- | --- | --- |
| **FEATURES**  Name:  Colour:  Installation:  Application: | | Track wall light  Matt black  Magnetic  Indoor |
| CCT:  Ra:  LED Chip:  Beam Angle:  Lumen: | 3000K/4000K/5000k  ≧90  OSRAM  120°  270lm | |
| **AVAILABLE** **MODELS** | | |
| Item | Power(w) | Size(mm) |
| EM-EH-CWL-5 | 5 | ø180\*H23 |