**IP20**

**TECHNICAL IMAGE**



**DESIGN** **BY**

Emilux Lighting Limited

**DESCRIPTION**

* Multi power for commercial and architectural lighting
* Average lighting with die-casting Aluminium material
* Average performance within different dimension
* External dimming system: Triac/ 0-10V/ Dali/Bluetooth/ Tuya/ Zigbee

|  |  |
| --- | --- |
| **FEATURES**Name:Colour:Installation:Application: | Track wall lightMatt blackMagneticIndoor |
| CCT:Ra:LED Chip:Beam Angle:Lumen: | 3000K/4000K/5000k≧90OSRAM120°270lm |
| **AVAILABLE** **MODELS** |
| Item | Power(w) | Size(mm) |
| EM-EH-CWL-5 | 5 | ø180\*H23 |